# Assembly

1. Tin all surface mount pads
2. Place U1 and hot air into place
3. Place C1 and hot air into place
4. Hand solder J1. The notch should face outward
5. Hand solder J2. The notch should face outward